mFRR Standard Product (Energy Market)
Unofficial translation
	Parameter
	Condition

	Mode of activation

	Manual
The activation message is sent electronically from the System Operator’s balance management system.

	Activation type

	Direct or scheduled

	Full activation time (FAT)

	Up to 12.5 minutes

	Minimum quantity

	1 MW

	Bid granularity

	1 MW

	Maximum quantity

	9,999 MW, but not more than the prequalified volume

	Minimum duration of delivery period

	5 minutes

	Minimum duration of delivery period

	Up to 20 minutes for scheduled activation
Up to 35 minutes for direct activation

	Price resolution

	0.01 €/MWh

	Validity period

	Scheduled activation may occur only at the designated time.
Direct activation may occur at any time within 15 minutes after the scheduled time and the delivery of balancing energy continues until the end of the next trading period.


	Price of the bid

	Unit: €/MWh
The minimum and maximum prices are defined by the MARI balancing platform’s price limits.

	Divisibility
	Fully divisible bids in 1 MW steps, partially divisible bids,




	
	and fully indivisible bids are allowed.
The indivisible portion of a bid must not exceed the maximum amount fixed during prequalification.

	Direction

	Upward or downward

	Location

	Bidding zone

	Technical linking between bids

	Two mFRR energy bids on consecutive trading periods may be technically linked.

If a direct activation occurred in the previous trading period, the current bid is made unavailable for both direct and scheduled activation.

Bids can be simultaneously linked both technically and conditionally. Technical linking is allowed for both simple and complex bids.

	Conditional linking between bids

	The Balancing Service Provider may conditionally link mFRR energy bids.
Each bid has a preliminary status, which changes depending on whether the specified conditions are met.


	Preparation period
Preparation time is the time between start of preparation period and ramping period.
	No more than 7 minutes.
Exceptions are allowed if activation remains within the tolerance specified in the prequalification documentation.


	Ramping period

Ramping period is the time for BSP to change its resource unit’s output from initial set-point to the desired power output.
	No more than 12 minutes.
Exceptions are allowed if activation remains within the tolerance specified in the prequalification documentation.


	Deactivation Period

	Up to 10 minutes



	Deactivation period is the time for BSP to change its resource unit’s output from desired power output to its initial scheduled power output.
	

	Minimum duration between the end of deactivation and the following activation

	None



mFRR Standard Product (Capacity Market)
	Parameter
	Condition

	Direction

	Upward or downward

	Validity period

	1MTU (15 minutes)

	Minimum quantity

	1 MW

	Bid granularity

	1 MW

	Maximum quantity

	9,999 MW, but not more than the prequalified volume

	Divisibility
	Divisible in steps of 1 MW or indivisible, in accordance with the conditions set during prequalification and as specified in the Capacity Market Rules


	Volume

	Unit: MW

	Price of the bid

	Unit: €/MWh
Minimum and maximum prices are defined by the Baltic balancing capacity platform price limits


	Location

	Bidding zone

	Availability
	When submitting bids to the capacity market, technical constraints may be specified, such as divisibility,




	
	maximum consecutive operating time, and minimum pause between two accepted capacity bids, in accordance with the Capacity Market Rules.
mFRR energy bids must be fully available and ready for activation throughout the validity period of the accepted capacity offer, in at least the offered volume, as per standard product conditions.


The obligation to submit mFRR bids may be transferred to another prequalified Balancing Service Provider within the control area of the System Operator, in accordance with the Capacity Market Rules.


	Links between bids

	Linking of bids is permitted as follows:
· Block bids
Offers with the same direction, volume, and price across consecutive trading periods may be linked into one block bid. In such case, either all block-linked bids shall be accepted in the same volume, or all bids shall be rejected.
· Direction-linked bids
A bid may be linked within the same trading period to another bid for the same service. Such linked bids shall be accepted or rejected as a whole in the same volume.
· Mutually exclusive bids
A bid may be submitted as a bid curve consisting of up to 10 sub-bids, of which at most one sub-bid may be accepted.
Attention! Complex bids may be linked as mutually exclusive. Such bids may include block bids and direction-linked bids.


	Price method

	Marginal pricing



