FCR Capacity Market Standard Product
Unofficial translation
	Parameter
	Condition

	Mode of activation

	Automatic – the reserve unit autonomously determines the quantity to be activated based on the measured frequency deviation and the accepted capacity offer.

	Full activation time (FAT)

	30 seconds

	Direction

	Symmetric – both upward and downward

	Validity period

	15 minutes

	Minimum quantity

	1 MW

	Minimum duration of delivery period

	None

	Bid granularity

	1 MW

	Maximum quantity

	9,999 MW

	Divisibility
	Fully divisible in steps of 1 MW, fully indivisible, or partially indivisible in steps of 1 MW.


	Volume

	Unit: MW

	Price of the bid

	Unit: €/MWh

	Availability

	The FCR service must be fully available and ready for activation during the validity period of the accepted FCR offer, in at least the volume of the accepted capacity offer.
The obligation to submit the FCR offer may be transferred to another prequalified Balancing Service Provider within the TSO control area, in accordance with Article 34 of the EBGL Regulation.



	Links between bids

	Linking of bids is permitted as follows:
· Block bids
Offers with the same volume and price across consecutive trading periods may be linked into one block bid.
 In such cases, either all linked bids are accepted or all are rejected.

	Minimum duration between the end of deactivation and the following activation

	None

	Price method

	Marginal pricing



