aFRR Standard Product (Energy Market)
Unofficial translation
	Parameter
	Condition

	Mode of activation

	Automatic
The setpoint is continuously sent to the reserve unit via the System Operator’s SCADA. Activation takes place in steps of 0.1 MW.

	Full activation time (FAT)

	5 minutes

	Minimum quantity

	1 MW

	Bid granularity

	1 MW

	Maximum quantity

	9,999 MW

	Minimum duration of delivery period

	None

	Price resolution

	0.01 €/MWh

	Validity period

	15 minutes; the first validity period of the day starts at 00:00 CET. All validity periods are consecutive and non-overlapping.

	Price of the bid

	Unit: €/MWh

	Bidding zone

	The bidding zone in which the reserve unit or group is located.

	Divisibility

	Fully divisible in steps of 0.1 MW

	Direction

	Upward or downward

	Links between bids

	Linking of aFRR energy bids is not permitted.



	Preparation period

	Up to 30 seconds

	Ramping period

	Up to 5 minutes, including the preparation period

	Deactivation Period

	Up to 5 minutes

	Minimum duration of delivery period

	15 minutes

	Minimum duration between the end of deactivation and the following activation

	None



aFRR Standard Product (Capacity Market)
	Parameter
	Condition

	Direction

	Upward or downward

	Validity period

	1MTU (15 minutes)

	Minimum quantity

	1 MW

	Bid granularity

	1 MW

	Maximum quantity

	9,999 MW, but not more than the prequalified volume

	Divisibility
	Divisible in steps of 1 MW or indivisible, in accordance with the conditions set during prequalification and as specified in the Capacity Market Rules


	Volume

	Unit: MW

	Price of the bid

	Unit: €/MWh

	Location

	Bidding zone

	Availability

	When submitting bids to the capacity market, technical constraints may be defined such as divisibility, maximum consecutive operating time, and minimum pause between two accepted capacity offers, in accordance with the Capacity Market Rules.

aFRR energy bids must be fully available and ready for activation during the validity period of the accepted aFRR offer, in at least the volume of the accepted capacity offer.

The obligation to submit aFRR offers may be transferred to another prequalified Balancing Service Provider in accordance with the Capacity Market Rules.



	
	

	Links between bids

	Linking of bids is permitted as follows:
· Block bids
Offers with the same direction, volume, and price across consecutive trading periods may be linked into one block bid. In such cases, either all linked bids are accepted or all are rejected.
· Linked bids
Bids may be linked within the same trading period. Such linked bids shall be accepted or rejected as a whole in the same volume.

· Mutually exclusive bids
A bid may be submitted as part of a bid curve, from which at most one bid may be accepted. Mutually exclusive linking between aFRR and mFRR capacity bids is not permitted.


· Groups of mutually exclusive bids
Such groups may include block bids and linked bids. Up to 10 groups of bids may be submitted within one mutually exclusive group.


	Price method

	Marginal pricing



